Tools to rescue an IDU by flashing software into it.

1) Unzip the archive into a folder on your Windows laptop.
2) Double click on the "rescue-me.bat" script.
3) Connect an ethernet cable from the laptop to the Ethernet (not PoE)
   jack on the IDU.
4) Power up the IDU.
5) Wait 3-4 minutes until the IDU led starts slowly blinking red and
   green indicating it is done installing.
6) Power the IDU off and disconnect the ethernet cable.
7) Dismiss the tftp window on the laptop.
8) Power up the IDU and it should boot up normally.

Afterwards, we recommend doing an update right away from the Winegard
update server (WinegardConnect.com) to get the latest software.
This kit was tested on a Windows 7 laptop.

The additional "rescue_xxx.bin" images can be used to force the
board type as reflected in their name. By renaming the appropriate
one to "rescue.bin", it wil set the board type before installing
the new firmware. Normally, this isn't necessary but boards with
older bootloaders may require this.
